|  |
| --- |
| **ESTIMATE FOR AC**  |
|  | **FOR PUNJAB GRAMIN BANK, RO OFFICE , SUNNY ENCLAVE, Mohali** |
| **S.N** | **Descriptions of items** | **Qty** | **Unit** | **Rate** | **Amount** |
|  |  |  |  | **In Rs.**  | **In Rs.** |
| **1.** | **AC SPLIT (1.5 TON) – O.G. , DAKIN, HITACHI**  | 9 | Nos |  |  |
|  | Providing & Fixing of 1.5 ton Inverter AC with stand , stabilizer & 10’-0” AC pipe complete fitting.  |  |  |  |  |
| **2.** | **RE- FIXING AC**  | 3 | Nos |  |  |
|  | Removing of existing AC from old office and re-fixing at new office with gas filling & stand, with complete fitting. |  |  |  |  |
| **3.** | **AC COPPER PIPE**  | 400 | Rft. |  |  |
|  | Laying of AC copper pipe including cutting of walls and repair the same with the surface of walls. Copper pipe include 1/4" + 1/2 " & 3 core copper wire 2.5 sq mm in 1/2" flexible pipe properly insulated complete in all respect. Copper pipe/ wire should not be more than 2'-0" in length near outer unit. Pipe should be of total line co.  |  |  |  |  |
| **4..** | **AC DRAINAGE PIPE**  | 250 | Rft. |  |  |
|  | Drainage pipe for AC 25 mm PVC pipe of supreme co. including fitting. Wall cutting and repair with cement mortar.  |  |  |  |  |
|  | **TOTAL** |  |  |  |  |

**NOTE:**

**CONTARCTOR SHALL SUBMIT BILL OF THE AC COMPANY THAT AC USED ARE INVETER AC AND GENIUNE OF THE COMPANY WITH Guarantee CARD. OTHERWISE NO BILL OF CONTACTOR SHALL BE PASSED.**